GAS/OXYGEN CYLINDER INSPECTION

|  |  |  |  |
| --- | --- | --- | --- |
| SITE: |  | USER: |  |
| DATE: |  | TIME: |  |

|  |  |  |
| --- | --- | --- |
| **Item No.** | **Item Details** | **YES / NO / NA** |
|  | STORAGE |  |
| 1 | Stored in a cool well-ventilated area |  |
| 2 | Stored in an upright position |  |
| 3 | Each cylinder is individually chained |  |
| 4 | Stored on a level fireproof surface |  |
| 5 | Protected from direct sunlight |  |
| 6 | Protected from rain |  |
| 7 | Protected from corrosive substances |  |
| 8 | Storage area has symbolic signage installed |  |
| 9 | Signage: No smoking, open flames |  |
| 10 | Full and empty cylinders stored separately |  |
| 11 | LPGas over 18kg stored in outside area |  |
| 12 | LPGas stored outside weather protected |  |
| 13 | Oxygen stored separately |  |
| 14 | Oxygen isolated from flammable gas |  |
| 15 | Oxygen isolated from heat |  |
|  | CYLINDER |  |
| 16 | Equipped with valve protectors |  |
| 17 | Cylinder contents are easily identified |  |
| 18 | Cylinder not defaced |  |
| 19 | Cylinder casing has all required legal markings |  |
| 20 | Empty cylinders marked "Empty" or "MT" |  |
| 21 | Empty cylinders marked "Empty" or "MT" |  |
| 22 | Off-loaded in upright position |  |
| 23 | Used in upright position |  |
| 24 | Used in upright position |  |
| 25 | Not lifted by the neck during on/off loading |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# USER SIGNATURE